MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

Public Attributes | List of all members
_MWCAP_VIDEO_BUFFER_INFO Struct Reference
Structures

MWCAP_VIDEO_BUFFER_INFO. More...

`#include <MWCaptureExtension.h>`

## Public Attributes
DWORD | cMaxFrames
| Maximum number of frames in on-board cache.
BYTE | iNewestBuffering
| The number of the slices being bufferred. A frame of video data may contain multiple slices.
BYTE | iBufferingFieldIndex
| The sequence number of fields being bufferred.
BYTE | iNewestBuffered
| The sequence number of slices the latest bufferred piece.
BYTE | iBufferedFieldIndex
| The sequence number of the latest bufferred field.
BYTE | iNewestBufferedFullFrame
| The sequence number of the latest bufferred frame.
DWORD | cBufferedFullFrames
| Number of fully bufferred full frames.

## Detailed Description

MWCAP_VIDEO_BUFFER_INFO.

Records video buffer information.
Related functions are:
MWGetVideoBufferInfo

The documentation for this struct was generated from the following file:

- /Users/magewell/builds/ks3341Bc/0/msdk/research/mw_capture_sdk_mac/Include/LibMWCapture/MWCaptureExtension.h