MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

Public Attributes | List of all members
_MWCAP_PRO_CAPTURE_INFO Struct Reference
Structures

MWCAP_PCIE_CAPTURE_INFO. More...

`#include <MWCaptureExtension.h>`

## Public Attributes
BYTE | byPCIBusID
| PCIE bus id.
BYTE | byPCIDevID
| PCIE device id.
BYTE | byLinkType
| PCIE connection type, refers to _MWCAP_PCIE_LINK_TYPE.
BYTE | byLinkWidth
| PCIE bandwidth.
BYTE | byBoardIndex
| Capture board index, which is the same as the rotary number.
WORD | wMaxPayloadSize
| PCIE max payload.
WORD | wMaxReadRequestSize
| PCIE Max Read Request.
DWORD | cbTotalMemorySize
| PCIE total memory size.
DWORD | cbFreeMemorySize
| PCIE free memory size.

## Detailed Description

MWCAP_PCIE_CAPTURE_INFO.

Records PCIE connctions.
Related functions are:
MWGetFamilyInfoByIndex
MWGetFamilyInfo

The documentation for this struct was generated from the following file:

- /Users/magewell/builds/ks3341Bc/0/msdk/research/mw_capture_sdk_mac/Include/LibMWCapture/MWCaptureExtension.h