MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

Public Attributes | List of all members
_MWCAP_VIDEO_SIGNAL_STATUS Struct Reference
Structures

MWCAP_VIDEO_SIGNAL_STATUS. More...

`#include <MWCaptureExtension.h>`

## Public Attributes
MWCAP_VIDEO_SIGNAL_STATE | state
| Defines the accessibility of this video signal.
int | x
| Horizontal start position.
int | y
| Vertical start position.
int | cx
| Image width.
int | cy
| Image height.
int | cxTotal
| Total width.
int | cyTotal
| Total height.
BOOLEAN | bInterlaced
| Whether the signal is interlaced.
DWORD | dwFrameDuration
| Frame interval of video frame.
int | nAspectX
| Width of video ratio.
int | nAspectY
| Height of video ratio.
BOOLEAN | bSegmentedFrame
| Whether the signal is segmented frame.
MWCAP_VIDEO_FRAME_TYPE | frameType
| video frame type
MWCAP_VIDEO_COLOR_FORMAT | colorFormat
| video color format
MWCAP_VIDEO_QUANTIZATION_RANGE | quantRange
| Quantization range.
MWCAP_VIDEO_SATURATION_RANGE | satRange
| saturation range

## Detailed Description

MWCAP_VIDEO_SIGNAL_STATUS.

Defines video signal status.
Related functions are:
MWGetVideoSignalStatus

The documentation for this struct was generated from the following file:

- /Users/magewell/builds/ks3341Bc/0/msdk/research/mw_capture_sdk_mac/Include/LibMWCapture/MWCaptureExtension.h