MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

Public Attributes | List of all members
_MWCAP_HDMI_VIDEO_TIMING Struct Reference
Structures

MWCAP_HDMI_VIDEO_TIMING. More...

`#include <MWCaptureExtension.h>`

## Public Attributes
BOOLEAN | bInterlaced
| Whether the signal is interlaced.
DWORD | dwFrameDuration
| Frame time interval.
WORD | wHSyncWidth
| Horizontal sync width.
WORD | wHFrontPorch
| Horizontal front porch.
WORD | wHBackPorch
| Horizontal back porch.
WORD | wHActive
| Horizontal active width.
WORD | wHTotalWidth
| Horizontal total width.
WORD | wField0VSyncWidth
| Vertical sync width of top subframe.
WORD | wField0VFrontPorch
| Vertical front porch of top subframe.
WORD | wField0VBackPorch
| Vertical back porch of top subframe.
WORD | wField0VActive
| Vertical active width of top subframe.
WORD | wField0VTotalHeight
| Vertical total width of top subframe.
WORD | wField1VSyncWidth
| Vertical sync width of bottom subframe.
WORD | wField1VFrontPorch
| Vertical front porch of bottom subframe.
WORD | wField1VBackPorch
| Vertical back porch of bottom subframe.
WORD | wField1VActive
| Vertical active width of bottom subframe.
WORD | wField1VTotalHeight
| Vertical total width of bottom subframe.

## Detailed Description

MWCAP_HDMI_VIDEO_TIMING.

Records HDMI timing.
Related data type are
MWCAP_HDMI_SPECIFIC_STATUS
MWCAP_INPUT_SPECIFIC_STATUS
Related functions is:
MWGetInputSpecificStatus

The documentation for this struct was generated from the following file:

- /Users/magewell/builds/ks3341Bc/0/msdk/research/mw_capture_sdk_mac/Include/LibMWCapture/MWCaptureExtension.h