MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

Public Attributes | List of all members
_MWCAP_INPUT_SPECIFIC_STATUS Struct Reference
Structures

MWCAP_INPUT_SPECIFIC_STATUS. More...

`#include <MWCaptureExtension.h>`

## Public Attributes
BOOLEAN | bValid
| Whether input signal is valid.
DWORD | dwVideoInputType
| Input video signal type. For details, refers to MWCAP_VIDEO_INPUT_TYPE.
union {
MWCAP_SDI_SPECIFIC_STATUS sdiStatus
| SDI signal status.
MWCAP_HDMI_SPECIFIC_STATUS hdmiStatus
| HDMI signal status.
MWCAP_COMPONENT_SPECIFIC_STATUS vgaComponentStatus
| VGA component signal status.
MWCAP_CVBS_YC_SPECIFIC_STATUS cvbsYcStatus
| CVBS-YC signal status.
}; |

## Detailed Description

MWCAP_INPUT_SPECIFIC_STATUS.

Records input signal status.
Related functions are:
MWGetInputSpecificStatus

The documentation for this struct was generated from the following file:

- /Users/magewell/builds/ks3341Bc/0/msdk/research/mw_capture_sdk_mac/Include/LibMWCapture/MWCaptureExtension.h