MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

Public Attributes | List of all members
_MWCAP_AUDIO_CAPTURE_FRAME Struct Reference
Structures

MWCAP_AUDIO_CAPTURE_FRAME. More...

`#include <MWCaptureExtension.h>`

## Public Attributes
DWORD | cFrameCount
| Number of bufferred frames.
DWORD | iFrame
| Current frame index.
DWORD | dwSyncCode
| Sync code of audio frame data.
DWORD | dwReserved
| Reserved.
LONGLONG | llTimestamp
| The timestamp of audio frame.
DWORD | adwSamples [MWCAP_AUDIO_SAMPLES_PER_FRAME *MWCAP_AUDIO_MAX_NUM_CHANNELS]
| Audio sample data. Each sample is 32-bit width, and high bit effective. The priority of the path is: Left0, Left1, Left2, Left3, right0, right1, right2, right3.

## Detailed Description

MWCAP_AUDIO_CAPTURE_FRAME.

Records audio frame info.
Related functions are:
MWCaptureAudioFrame

The documentation for this struct was generated from the following file:

- /Users/magewell/builds/ks3341Bc/0/msdk/research/mw_capture_sdk_mac/Include/LibMWCapture/MWCaptureExtension.h