MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

Public Attributes | List of all members
_MWCAP_AUDIO_SIGNAL_STATUS Struct Reference
Structures

MWCAP_AUDIO_SIGNAL_STATUS. More...

`#include <MWCaptureExtension.h>`

## Public Attributes
WORD | wChannelValid
| Valid audio channel mask.The lowest bit indicates whether the 1st and 2nd channels are valid, the second bit indicates whether the 3rd and 4th channels are valid, the third bit indicates whether the 5th and 6th channels are valid, and the fourth bit indicates whether the 7th and 8th channels are valid.
BOOLEAN | bLPCM
| Whether the signal is LPCM.
BYTE | cBitsPerSample
| Bit depth of each audio sampling.
DWORD | dwSampleRate
| Sample rate.
BOOLEAN | bChannelStatusValid
| Whether channel status is valid.
IEC60958_CHANNEL_STATUS | channelStatus
| The audio channel status.

## Detailed Description

MWCAP_AUDIO_SIGNAL_STATUS.

Records audio signal status.
Related functions is
MWGetAudioSignalStatus

The documentation for this struct was generated from the following file:

- /Users/magewell/builds/ks3341Bc/0/msdk/research/mw_capture_sdk_mac/Include/LibMWCapture/MWCaptureExtension.h