MWCapture SDK Mac 3.4.62314

- Home
- Development Library
- Release Notes

MWHDMIPackets.h
1
2// CONFIDENTIAL and PROPRIETARY software of Magewell Electronics Co., Ltd.
3// Copyright (c) 2011-2014 Magewell Electronics Co., Ltd. (Nanjing)
4// All rights reserved.
5// This copyright notice MUST be reproduced on all authorized copies.
7
8#pragma once
9
10#pragma pack(push)
11#pragma pack(1)
12
13// AVI infoframe
14#define HDMI_EC_XVYCC601 0x00
15#define HDMI_EC_XVYCC709 0x01
16#define HDMI_EC_SYCC601 0x02
17#define HDMI_EC_ADOBEYCC601 0x03
18#define HDMI_EC_ADOBERGB 0x04
19
20#define HDMI_YQ_LIMITED_RANGE 0x00
21#define HDMI_YQ_FULL_RANGE 0x01
22
23#define HDMI_CN_NONE_OR_GRAPHICS 0x00
24#define HDMI_CN_PHOTO 0x01
25#define HDMI_CN_CINEMA 0x02
26#define HDMI_CN_GAME 0x03
27
28 typedef struct _HDMI_VIC_FORMAT {
29 WORD cx;
30 WORD cy;
31 BOOLEAN bInterlaced;
32 WORD wAspectX;
33 WORD wAspectY;
34 DWORD dwFrameDuration;
35} HDMI_VIC_FORMAT;
36
37 static const HDMI_VIC_FORMAT g_aHDMIVICFormats[] = {
38 /* 0 */ { 0, 0, FALSE, 0, 0, 0, },
39 /* 1 */ { 640, 480, FALSE, 4, 3, 166667, },
40 /* 2 */ { 720, 480, FALSE, 4, 3, 166667, },
41 /* 3 */ { 720, 480, FALSE, 16, 9, 166667, },
42 /* 4 */ { 1280, 720, FALSE, 16, 9, 166667, },
43 /* 5 */ { 1920, 1080, TRUE, 16, 9, 333333, },
44 /* 6 */ { 720, 480, TRUE, 4, 3, 333333, },
45 /* 7 */ { 720, 480, TRUE, 16, 9, 333333, },
46 /* 8 */ { 720, 240, FALSE, 4, 3, 166667, },
47 /* 9 */ { 720, 240, FALSE, 16, 9, 166667, },
48 /* 10 */ { 2880, 480, TRUE, 4, 3, 333333, },
49 /* 11 */ { 2880, 480, TRUE, 16, 9, 333333, },
50 /* 12 */ { 2880, 240, FALSE, 4, 3, 166667, },
51 /* 13 */ { 2880, 240, FALSE, 16, 9, 166667, },
52 /* 14 */ { 1440, 480, FALSE, 4, 3, 166667, },
53 /* 15 */ { 1440, 480, FALSE, 16, 9, 166667, },
54 /* 16 */ { 1920, 1080, FALSE, 16, 9, 166667, },
55 /* 17 */ { 720, 576, FALSE, 4, 3, 200000, },
56 /* 18 */ { 720, 576, FALSE, 16, 9, 200000, },
57 /* 19 */ { 1280, 720, FALSE, 16, 9, 200000, },
58 /* 20 */ { 1920, 1080, TRUE, 16, 9, 400000, },
59 /* 21 */ { 720, 576, TRUE, 4, 3, 400000, },
60 /* 22 */ { 720, 576, TRUE, 16, 9, 400000, },
61 /* 23 */ { 720, 288, FALSE, 4, 3, 200000, },
62 /* 24 */ { 720, 288, FALSE, 16, 9, 200000, },
63 /* 25 */ { 2880, 576, TRUE, 4, 3, 400000, },
64 /* 26 */ { 2880, 576, TRUE, 4, 3, 400000, },
65 /* 27 */ { 2880, 288, FALSE, 4, 3, 200000, },
66 /* 28 */ { 2880, 288, FALSE, 16, 9, 200000, },
67 /* 29 */ { 1440, 576, FALSE, 4, 3, 200000, },
68 /* 30 */ { 1440, 576, FALSE, 16, 9, 200000, },
69 /* 31 */ { 1920, 1080, FALSE, 16, 9, 200000, },
70 /* 32 */ { 1920, 1080, FALSE, 16, 9, 416667, },
71 /* 33 */ { 1920, 1080, FALSE, 16, 9, 400000, },
72 /* 34 */ { 1920, 1080, FALSE, 16, 9, 333333, },
73 /* 35 */ { 2880, 480, FALSE, 4, 3, 166667, },
74 /* 36 */ { 2880, 480, FALSE, 16, 9, 166667, },
75 /* 37 */ { 2880, 576, FALSE, 4, 3, 200000, },
76 /* 38 */ { 2880, 576, FALSE, 16, 9, 200000, },
77 /* 39 */ { 1920, 1080, TRUE, 16, 9, 400000, },
78 /* 40 */ { 1920, 1080, TRUE, 16, 9, 200000, },
79 /* 41 */ { 1280, 720, FALSE, 16, 9, 100000, },
80 /* 42 */ { 720, 576, FALSE, 4, 3, 100000, },
81 /* 43 */ { 720, 576, FALSE, 16, 9, 100000, },
82 /* 44 */ { 720, 576, TRUE, 4, 3, 200000, },
83 /* 45 */ { 720, 576, TRUE, 16, 9, 200000, },
84 /* 46 */ { 1920, 1080, TRUE, 16, 9, 166667, },
85 /* 47 */ { 1280, 720, FALSE, 16, 9, 83333, },
86 /* 48 */ { 720, 480, FALSE, 4, 3, 83333, },
87 /* 49 */ { 720, 480, FALSE, 16, 9, 83333, },
88 /* 50 */ { 720, 480, TRUE, 4, 3, 166667, },
89 /* 51 */ { 720, 480, TRUE, 16, 9, 166667, },
90 /* 52 */ { 720, 576, FALSE, 4, 3, 50000, },
91 /* 53 */ { 720, 576, FALSE, 16, 9, 50000, },
92 /* 54 */ { 720, 576, TRUE, 4, 3, 100000, },
93 /* 55 */ { 720, 576, TRUE, 16, 9, 100000, },
94 /* 56 */ { 720, 480, FALSE, 4, 3, 41667, },
95 /* 57 */ { 720, 480, FALSE, 16, 9, 41667, },
96 /* 58 */ { 720, 480, TRUE, 4, 3, 83333, },
97 /* 59 */ { 720, 480, TRUE, 16, 9, 83333, },
98 /* 60 */ { 1280, 720, FALSE, 16, 9, 416667, },
99 /* 61 */ { 1280, 720, FALSE, 16, 9, 400000, },
100 /* 62 */ { 1280, 720, FALSE, 16, 9, 333333, },
101 /* 63 */ { 1920, 1080, FALSE, 16, 9, 83333, },
102 /* 64 */ { 1920, 1080, FALSE, 16, 9, 100000 },
103};
104
105 static const HDMI_VIC_FORMAT g_aHDMIExtVICFormats[] = {
106 /* 0 */ { 0, 0, FALSE, 0, 0, 0, },
107 /* 1 */ { 3840, 2160, FALSE, 16, 9, 333333, },
108 /* 2 */ { 3840, 2160, FALSE, 16, 9, 400000, },
109 /* 3 */ { 3840, 2160, FALSE, 16, 9, 416667, },
110 /* 4 */ { 4096, 2160, FALSE, 16, 9, 416667 },
111};
112
113 static const BYTE g_abyDefaultYUV709VICs[] = {
114 0, 1, 4, 5, 16, 19, 20, 31, 32, 33, 34, 39, 40, 46, 47, 60, 61, 62, 63, 64
115};
116
117// byRGB_YCbCr
118 typedef enum _HDMI_PIXEL_ENCODING {
119 HDMI_ENCODING_RGB_444 = 0,
120 HDMI_ENCODING_YUV_422 = 1,
121 HDMI_ENCODING_YUV_444 = 2,
122 HDMI_ENCODING_YUV_420 = 3
123} HDMI_PXIEL_ENCODING;
124
130 typedef struct _HDMI_AVI_INFOFRAME_PAYLOAD {
131 BYTE byScanInfo : 2;
132 BYTE byBarDataPresent : 2;
133 BYTE byActiveFormatInfoPresent : 1;
134 BYTE byRGB_YCbCr : 2;
135 BYTE byFutureUseByte1 : 1;
136
137 BYTE byActivePortionAspectRatio : 4;
138 BYTE byCodedFrameAspectRatio : 2;
139 BYTE byColorimetry : 2;
140
141 BYTE byNonUniformPictureScaling : 2;
142 BYTE byRGBQuantizationRange : 2;
143 BYTE byExtendedColorimetry : 3;
144 BYTE byITContent : 1;
145
146 BYTE byVIC : 7;
147 BYTE byFutureUseByte4 : 1;
148
149 BYTE byPixelRepetitionFactor : 4;
150 BYTE byITContentType : 2;
151 BYTE byYCCQuantizationRange : 2;
152
153 WORD wEndOfTopBar;
154 WORD wStartOfBottomBar;
155 WORD wEndOfLeftBar;
156 WORD wStartOfRightBar;
157} HDMI_AVI_INFOFRAME_PAYLOAD;
158
159 typedef struct _HDMI_HDR_INFOFRAME_PAYLOAD {
160 BYTE byEOTF;
161 BYTE byMetadataDescriptorID;
162
163 BYTE display_primaries_lsb_x0;
164 BYTE display_primaries_msb_x0;
165 BYTE display_primaries_lsb_y0;
166 BYTE display_primaries_msb_y0;
167
168 BYTE display_primaries_lsb_x1;
169 BYTE display_primaries_msb_x1;
170 BYTE display_primaries_lsb_y1;
171 BYTE display_primaries_msb_y1;
172
173 BYTE display_primaries_lsb_x2;
174 BYTE display_primaries_msb_x2;
175 BYTE display_primaries_lsb_y2;
176 BYTE display_primaries_msb_y2;
177
178 BYTE white_point_lsb_x;
179 BYTE white_point_msb_x;
180 BYTE white_point_lsb_y;
181 BYTE white_point_msb_y;
182
183 BYTE max_display_mastering_lsb_luminance;
184 BYTE max_display_mastering_msb_luminance;
185 BYTE min_display_mastering_lsb_luminance;
186 BYTE min_display_mastering_msb_luminance;
187
188 BYTE maximum_content_light_level_lsb;
189 BYTE maximum_content_light_level_msb;
190
191 BYTE maximum_frame_average_light_level_lsb;
192 BYTE maximum_frame_average_light_level_msb;
193} HDMI_HDR_INFOFRAME_PAYLOAD;
194
195
196// Audio infoframe
197#define HDMI_AUDIO_CODING_TYPE_STREAM 0x00
198#define HDMI_AUDIO_CODING_TYPE_PCM 0x01
199#define HDMI_AUDIO_CODING_TYPE_AC3 0x02
200#define HDMI_AUDIO_CODING_TYPE_MPEG1 0x03
201#define HDMI_AUDIO_CODING_TYPE_MP3 0x04
202#define HDMI_AUDIO_CODING_TYPE_MPEG2 0x05
203#define HDMI_AUDIO_CODING_TYPE_AAC_LC 0x06
204#define HDMI_AUDIO_CODING_TYPE_DTS 0x07
205#define HDMI_AUDIO_CODING_TYPE_ATRAC 0x08
206#define HDMI_AUDIO_CODING_TYPE_DSD 0x09
207#define HDMI_AUDIO_CODING_TYPE_EAC3 0x0A
208#define HDMI_AUDIO_CODING_TYPE_DTS_HD 0x0B
209
210#define HDMI_AUDIO_SAMPLE_SIZE_STREAM 0x00
211#define HDMI_AUDIO_SAMPLE_SIZE_16BIT 0x01
212#define HDMI_AUDIO_SAMPLE_SIZE_20BIT 0x02
213#define HDMI_AUDIO_SAMPLE_SIZE_24BIT 0x03
214
215#define HDMI_AUDIO_SAMPLE_RATE_STREAM 0x00
216#define HDMI_AUDIO_SAMPLE_RATE_32000 0x01
217#define HDMI_AUDIO_SAMPLE_RATE_44100 0x02
218#define HDMI_AUDIO_SAMPLE_RATE_48000 0x03
219#define HDMI_AUDIO_SAMPLE_RATE_88200 0x04
220#define HDMI_AUDIO_SAMPLE_RATE_96000 0x05
221#define HDMI_AUDIO_SAMPLE_RATE_176400 0x06
222#define HDMI_AUDIO_SAMPLE_RATE_192000 0x07
223
224 typedef struct _HDMI_AUDIO_INFOFRAME_PAYLOAD {
225 BYTE byChannelCount : 3; // +1 for channel count
226 BYTE byReserved1 : 1;
227 BYTE byAudioCodingType : 4;
228
229 BYTE bySampleSize : 2;
230 BYTE bySampleFrequency : 3;
231 BYTE byReserved2 : 3;
232
233 BYTE byAudioCodingExtensionType : 5;
234 BYTE byReserved3 : 3;
235
236 BYTE byChannelAllocation;
237
238 BYTE byLFEPlaybackLevel : 2;
239 BYTE byReserved4 : 1;
240 BYTE byLevelShiftValue : 4;
241 BYTE byDownMixInhibitFlag : 1;
242} HDMI_AUDIO_INFOFRAME_PAYLOAD;
243
244// SPD Infoframe
245#define HDMI_SPD_SORUCE_UNKOWN 0x00
246#define HDMI_SPD_SORUCE_DIGITAL_STB 0x01
247#define HDMI_SPD_SORUCE_DVD_PLAYER 0x02
248#define HDMI_SPD_SORUCE_D_VHS 0x03
249#define HDMI_SPD_SORUCE_HDD_RECORDER 0x04
250#define HDMI_SPD_SORUCE_DVC 0x05
251#define HDMI_SPD_SORUCE_DSC 0x06
252#define HDMI_SPD_SORUCE_VIDEO_CD 0x07
253#define HDMI_SPD_SORUCE_GAME 0x08
254#define HDMI_SPD_SORUCE_PC_GENERAL 0x09
255#define HDMI_SPD_SORUCE_BLUE_RAY_DISC 0x0A
256#define HDMI_SPD_SORUCE_SUPER_AUDIO_CD 0x0B
257#define HDMI_SPD_SORUCE_HD_DVD 0x0C
258#define HDMI_SPD_SORUCE_PMP 0x0D
259
260 typedef struct _HDMI_SPD_INFOFRAME_PAYLOAD {
261 CHAR achVendorName[8];
262 CHAR achProductDescription[16];
263 BYTE bySourceInformation;
264} HDMI_SPD_INFOFRAME_PAYLOAD;
265
266// HDMI 1.4b VS Infoframe
267#define HDMI14B_VS_REGISTRATION_ID 0x000C03
268
269#define HDMI14B_VS_FORMAT_NONE 0x00
270#define HDMI14B_VS_FORMAT_EXT_RES 0x01
271#define HDMI14B_VS_FORMAT_3D_FORMAT 0x02
272
273// by3DStructure
274#define HDMI14B_3DS_FRAME_PACKING 0x00
275#define HDMI14B_3DS_FIELD_ALTERNATIVE 0x01
276#define HDMI14B_3DS_LINE_ALTERNATIVE 0x02
277#define HDMI14B_3DS_SIDE_BY_SIDE_FULL 0x03
278#define HDMI14B_3DS_TOP_AND_BOTTOM 0x06
279#define HDMI14B_3DS_SIDE_BY_SIDE_HALF 0x08
280
281// by3DExtData
282#define HDMI_SUB_SAMPLING_HORIZONTAL_00 0x00
283#define HDMI_SUB_SAMPLING_HORIZONTAL_01 0x01
284#define HDMI_SUB_SAMPLING_HORIZONTAL_10 0x02
285#define HDMI_SUB_SAMPLING_HORIZONTAL_11 0x03
286#define HDMI_SUB_SAMPLING_QUINCUNX_ODD_ODD 0x04
287#define HDMI_SUB_SAMPLING_QUINCUNX_ODD_EVEN 0x05
288#define HDMI_SUB_SAMPLING_QUINCUNX_EVEN_ODD 0x06
289#define HDMI_SUB_SAMPLING_QUINCUNX_EVEN_EVEN 0x07
290
291 typedef struct _HDMI14B_VS_DATA_EXT_RES {
292 BYTE byHDMI_VIC;
293} HDMI14B_VS_DATA_EXT_RES;
294
295 typedef struct _HDMI14B_VS_DATA_3D_FORMAT {
296 BYTE byReserved1 : 3;
297 BYTE by3DMetaPresent : 1;
298 BYTE by3DStructure : 4;
299
300 BYTE byReserved2 : 4;
301 BYTE by3DExtData : 4;
302
303 BYTE by3DMetadataLength : 5;
304 BYTE by3DMetadataType : 3;
305} HDMI14B_VS_DATA_3D_FORMAT;
306
307 typedef struct _HDMI14B_VS_DATA {
308 BYTE byReserved1 : 5;
309 BYTE byHDMIVideoFormat : 3;
310
311 union {
312 HDMI14B_VS_DATA_EXT_RES vsDataExtRes;
313 HDMI14B_VS_DATA_3D_FORMAT vsData3DFormat;
314 };
315} HDMI14B_VS_DATA;
316
317// Generic VS Infoframe
318 typedef struct _HDMI_VS_INFOFRAME_PAYLOAD {
319 BYTE abyRegistrationId[3];
320
321 union {
322 BYTE abyVSData[24];
323 HDMI14B_VS_DATA vsDataHDMI14B;
324 };
325} HDMI_VS_INFOFRAME_PAYLOAD;
326
327 static inline DWORD hdmi_payload_GetRegistrationId(HDMI_VS_INFOFRAME_PAYLOAD *payload)
328{
329 return payload->abyRegistrationId[0] | (payload->abyRegistrationId[1] << 8)
330 | (payload->abyRegistrationId[2] << 16);
331}
332
333// Generic Infoframe
334#define HDMI_INFOFRAME_TYPE_VS 0x81
335#define HDMI_INFOFRAME_TYPE_AVI 0x82
336#define HDMI_INFOFRAME_TYPE_SPD 0x83
337#define HDMI_INFOFRAME_TYPE_AUDIO 0x84
338#define HDMI_INFOFRAME_TYPE_MS 0x85
339#define HDMI_INFOFRAME_TYPE_VBI 0x86
340#define HDMI_INFOFRAME_TYPE_HDR 0x87
341
348 typedef struct _HDMI_INFOFRAME_HEADER {
349 BYTE byPacketType;
350 BYTE byVersion;
351 BYTE byLength : 5;
352 BYTE byReservedZero : 3;
353} HDMI_INFOFRAME_HEADER;
354
361 typedef struct _HDMI_INFOFRAME_PACKET {
362 HDMI_INFOFRAME_HEADER header;
363 BYTE byChecksum;
364
365 union {
366 BYTE abyPayload[27];
367 HDMI_AVI_INFOFRAME_PAYLOAD aviInfoFramePayload;
368 HDMI_AUDIO_INFOFRAME_PAYLOAD audioInfoFramePayload;
369 HDMI_SPD_INFOFRAME_PAYLOAD spdInfoFramePayload;
370 HDMI_VS_INFOFRAME_PAYLOAD vsInfoFramePayload;
371 HDMI_HDR_INFOFRAME_PAYLOAD hdrInfoFramePayload;
372 };
373} HDMI_INFOFRAME_PACKET;
374
375 static inline BOOLEAN hdmi_info_IsValid(HDMI_INFOFRAME_PACKET *info)
376{
377 unsigned char *pbyData = (unsigned char *)&info->header;
378 BYTE cbData = info->header.byLength + sizeof(info->header) + 1;
379
380 BYTE bySum = 0;
381 while (cbData-- != 0)
382 bySum += *pbyData++;
383
384 return (bySum == 0);
385}
386
387#pragma pack(pop)
388
HDMI_INFOFRAME_PACKET
struct _HDMI_INFOFRAME_PACKET HDMI_INFOFRAME_PACKET
HDMI_INFOFRAME_PACKET.
HDMI_INFOFRAME_HEADER
struct _HDMI_INFOFRAME_HEADER HDMI_INFOFRAME_HEADER
HDMI_INFOFRAME_HEADER.
HDMI_AVI_INFOFRAME_PAYLOAD
struct _HDMI_AVI_INFOFRAME_PAYLOAD HDMI_AVI_INFOFRAME_PAYLOAD
HDMI_AVI_INFOFRAME_PAYLOAD.
_HDMI14B_VS_DATA_3D_FORMAT
Definition: MWHDMIPackets.h:295
_HDMI14B_VS_DATA_EXT_RES
Definition: MWHDMIPackets.h:291
_HDMI14B_VS_DATA
Definition: MWHDMIPackets.h:307
_HDMI_AUDIO_INFOFRAME_PAYLOAD
Definition: MWHDMIPackets.h:224
_HDMI_AVI_INFOFRAME_PAYLOAD
HDMI_AVI_INFOFRAME_PAYLOAD.
Definition: MWHDMIPackets.h:130
_HDMI_AVI_INFOFRAME_PAYLOAD::byVIC
BYTE byVIC
Video identification code.
Definition: MWHDMIPackets.h:146
_HDMI_AVI_INFOFRAME_PAYLOAD::byRGBQuantizationRange
BYTE byRGBQuantizationRange
RGB quantization range.
Definition: MWHDMIPackets.h:142
_HDMI_AVI_INFOFRAME_PAYLOAD::byNonUniformPictureScaling
BYTE byNonUniformPictureScaling
Non-uniform picture ratio.
Definition: MWHDMIPackets.h:141
_HDMI_AVI_INFOFRAME_PAYLOAD::byYCCQuantizationRange
BYTE byYCCQuantizationRange
YCCC quantization range.
Definition: MWHDMIPackets.h:151
_HDMI_AVI_INFOFRAME_PAYLOAD::wStartOfRightBar
WORD wStartOfRightBar
Unsigned integer, representing the first pixel of the vertical letterbox bar on the right....
Definition: MWHDMIPackets.h:156
_HDMI_AVI_INFOFRAME_PAYLOAD::byPixelRepetitionFactor
BYTE byPixelRepetitionFactor
Pixel repetition factor.
Definition: MWHDMIPackets.h:149
_HDMI_AVI_INFOFRAME_PAYLOAD::wStartOfBottomBar
WORD wStartOfBottomBar
Unsigned integers represent the first line of the letterbox bar at the bottom of the horizontal scree...
Definition: MWHDMIPackets.h:154
_HDMI_AVI_INFOFRAME_PAYLOAD::byITContent
BYTE byITContent
IT content.
Definition: MWHDMIPackets.h:144
_HDMI_AVI_INFOFRAME_PAYLOAD::byCodedFrameAspectRatio
BYTE byCodedFrameAspectRatio
Frame Aspect Ratio.
Definition: MWHDMIPackets.h:138
_HDMI_AVI_INFOFRAME_PAYLOAD::byActiveFormatInfoPresent
BYTE byActiveFormatInfoPresent
Whether the active format is present.
Definition: MWHDMIPackets.h:133
_HDMI_AVI_INFOFRAME_PAYLOAD::byColorimetry
BYTE byColorimetry
Colorimetry,This field is used with Extended Colorimetry to indicate the color code of the video sour...
Definition: MWHDMIPackets.h:139
_HDMI_AVI_INFOFRAME_PAYLOAD::wEndOfTopBar
WORD wEndOfTopBar
Unsigned integers represent the last line of the letterbox bar area at the top of the screen....
Definition: MWHDMIPackets.h:153
_HDMI_AVI_INFOFRAME_PAYLOAD::byActivePortionAspectRatio
BYTE byActivePortionAspectRatio
Active Format Aspect Ratio.
Definition: MWHDMIPackets.h:137
_HDMI_AVI_INFOFRAME_PAYLOAD::byITContentType
BYTE byITContentType
IT content type.
Definition: MWHDMIPackets.h:150
_HDMI_AVI_INFOFRAME_PAYLOAD::byFutureUseByte1
BYTE byFutureUseByte1
Reserved.
Definition: MWHDMIPackets.h:135
_HDMI_AVI_INFOFRAME_PAYLOAD::byScanInfo
BYTE byScanInfo
scan information
Definition: MWHDMIPackets.h:131
_HDMI_AVI_INFOFRAME_PAYLOAD::byExtendedColorimetry
BYTE byExtendedColorimetry
Extended Colorimetry.
Definition: MWHDMIPackets.h:143
_HDMI_AVI_INFOFRAME_PAYLOAD::byRGB_YCbCr
BYTE byRGB_YCbCr
RGB or YCbCr.
Definition: MWHDMIPackets.h:134
_HDMI_AVI_INFOFRAME_PAYLOAD::wEndOfLeftBar
WORD wEndOfLeftBar
Unsigned integer, representing the last pixel of the vertical letterbox bar on the left....
Definition: MWHDMIPackets.h:155
_HDMI_AVI_INFOFRAME_PAYLOAD::byFutureUseByte4
BYTE byFutureUseByte4
Reserved.
Definition: MWHDMIPackets.h:147
_HDMI_AVI_INFOFRAME_PAYLOAD::byBarDataPresent
BYTE byBarDataPresent
Whether the Bar data is valid.
Definition: MWHDMIPackets.h:132
_HDMI_HDR_INFOFRAME_PAYLOAD
Definition: MWHDMIPackets.h:159
_HDMI_INFOFRAME_HEADER
HDMI_INFOFRAME_HEADER.
Definition: MWHDMIPackets.h:348
_HDMI_INFOFRAME_HEADER::byLength
BYTE byLength
length of infoframe
Definition: MWHDMIPackets.h:351
_HDMI_INFOFRAME_HEADER::byVersion
BYTE byVersion
HDMI version.
Definition: MWHDMIPackets.h:350
_HDMI_INFOFRAME_HEADER::byReservedZero
BYTE byReservedZero
Reserved.
Definition: MWHDMIPackets.h:352
_HDMI_INFOFRAME_HEADER::byPacketType
BYTE byPacketType
HDMI infoframe type.
Definition: MWHDMIPackets.h:349
_HDMI_INFOFRAME_PACKET
HDMI_INFOFRAME_PACKET.
Definition: MWHDMIPackets.h:361
_HDMI_INFOFRAME_PACKET::audioInfoFramePayload
HDMI_AUDIO_INFOFRAME_PAYLOAD audioInfoFramePayload
audio infoframe payload
Definition: MWHDMIPackets.h:368
_HDMI_INFOFRAME_PACKET::header
HDMI_INFOFRAME_HEADER header
HDMI infoframe header.
Definition: MWHDMIPackets.h:362
_HDMI_INFOFRAME_PACKET::abyPayload
BYTE abyPayload[27]
aby payload
Definition: MWHDMIPackets.h:366
_HDMI_INFOFRAME_PACKET::byChecksum
BYTE byChecksum
checksum
Definition: MWHDMIPackets.h:363
_HDMI_INFOFRAME_PACKET::spdInfoFramePayload
HDMI_SPD_INFOFRAME_PAYLOAD spdInfoFramePayload
spd infoframe payload
Definition: MWHDMIPackets.h:369
_HDMI_INFOFRAME_PACKET::hdrInfoFramePayload
HDMI_HDR_INFOFRAME_PAYLOAD hdrInfoFramePayload
hdr infoframe payload
Definition: MWHDMIPackets.h:371
_HDMI_INFOFRAME_PACKET::aviInfoFramePayload
HDMI_AVI_INFOFRAME_PAYLOAD aviInfoFramePayload
avi infoframe payload
Definition: MWHDMIPackets.h:367
_HDMI_INFOFRAME_PACKET::vsInfoFramePayload
HDMI_VS_INFOFRAME_PAYLOAD vsInfoFramePayload
vs infoframe payload
Definition: MWHDMIPackets.h:370
_HDMI_SPD_INFOFRAME_PAYLOAD
Definition: MWHDMIPackets.h:260
_HDMI_VIC_FORMAT
Definition: MWHDMIPackets.h:28
_HDMI_VS_INFOFRAME_PAYLOAD
Definition: MWHDMIPackets.h:318